CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.0/conf/instr/spect/uxnmr.info
Date         : Tue Nov 29 13:46:18 2022
Release      : TopSpin 3.6.0
Installed in : /opt/topspin3.6.0
Host         : av700
OS           : CentOS Linux release 7.5.1804 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 v4 @ 3.50GHz (8 cores at 1277 MHz with Hyperthreading)
User         : smvf (Stefan Freund)
System       : Avance III 700 NMR spectrometer
1H-frequency : 699.05 MHz
Description  : Avance III 700
Bruker Order : 11059545
Configured in: av700:/opt/topspin3.6.0/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.92
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/00452 ECL 03.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x3    AW  R  2.0 REC-1  AQS RXAD1000 Z102118/77 ECL 02.00
     3   0x34 0xc1   0x1        X  0.4 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x29   0x8    AE  S  3.0 SGU-1  AQS SGU/2 1000 Z103082/00428 ECL 03.00 FPGA-Vs=AF
     5   0x25 0x29   0x8    AE  S  2.0 SGU-2  AQS SGU/2 1000 Z103082/00117 ECL 02.00 FPGA-Vs=AF
     6   0x26 0x29   0x8    AE  S  2.0 SGU-3  AQS SGU/2 1000 Z103082/00134 ECL 02.00 FPGA-Vs=AF
     7   0x27 0x29   0x8    AE  S  2.0 SGU-4  AQS SGU/2 1000 Z103082/00132 ECL 02.00 FPGA-Vs=AF
    21   0x21 0xcf     0        P  0.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xc6     0        B  1.2 AQS/2  AQS/2 chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345092_0025 W1345092/0025 ECL 0:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ: W1345092/0025 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0108 ECL 0
- Controller     = BLA CONTROL BOARD 6 1V V-USB: W1522041/0085 ECL 1
BLA_W1345097_0016 W1345097/0016 ECL 0:
- TCP/IP address = 149.236.99.90
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ: W1345097/0016 ECL 0
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0083 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0204 ECL 1

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210921
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS2-SB
- 2HTX Amplifier: not available
- Lock: installed

Cryo Controller CRCO: device connected to 149.236.99.92:/dev/tty04

Eurotherm VTU: device connected to 149.236.99.92:/dev/tty01

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003463, SN=00135 from 20150311
    Module  2 : XBB19F 2HS
                PN=Z003507, SN=00101 from 20050208
    Module  3 : 2H
                PN=Z003474, SN=00087 from 20051031
    Module  4 : 13C
                PN=Z003525, SN=00069 from 20060403
    Module  5 : 15N
                PN=Z003531, SN=00064 from 20060411



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0016 at TCP/IP 149.236.99.90)
SGU1 AUX  output -> open
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0016 at TCP/IP 149.236.99.90)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0016 at TCP/IP 149.236.99.90)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAX300 E 6-365MHZ W1345092/0025 at TCP/IP 149.236.99.91)
SGU4 NORM output -> input 1 of transmitter 1 (BLAX300 E 6-365MHZ W1345092/0025 at TCP/IP 149.236.99.91)
SGU4 AUX  output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0016 at TCP/IP 149.236.99.90)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX300 E 6-365MHZ W1345092/0025 at TCP/IP 149.236.99.91:
- amplifier X-300W uses blanking 3

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ W1345097/0016 at TCP/IP 149.236.99.90:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking


