CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.5/conf/instr/700 AV III HD/uxnmr.info
Date         : Wed Jan  8 13:13:28 2025
Release      : TopSpin 3.6.5
Installed in : /opt/topspin3.6.5
Host         : CZC24393CF
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) W-2223 CPU @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Super User)
System       : Avance III HD 700 NMR spectrometer
1H-frequency : 698.88 MHz
Description  : Avance III
Configured in: CZC24393CF:/opt/topspin3.6.5/conf/instr/700 AV III HD

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.92
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/04552 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.3 REC-1  AQS RXAD/2 1000 Z130589/354 ECL 00.03
     3   0x34 0xda   0x1        X  2.2 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00495 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00496 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0781 W1345093/0781 ECL 12:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0781 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/3033 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/0233 ECL 50
BLA_W1345097_0345 W1345097/0345 ECL 20:
- TCP/IP address = 149.236.99.90
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0345 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/2530 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010482 ECL 50

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20230420
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS2-SB
- 2HTX Amplifier: not available
- Lock: installed
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/02530 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/02920 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.92:/dev/tty04

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : 1H LNA
                PN=Z003463, SN=00135 from 20150311
    Module  2 : XBB19F 2HS
                PN=Z003507, SN=00101 from 20050208
    Module  3 : 2H
                PN=Z003474, SN=00087 from 20051031
    Module  4 : 13C
                PN=Z003525, SN=00069 from 20060403
    Module  5 : 15N
                PN=Z003531, SN=00064 from 20060411



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0345 at TCP/IP 149.236.99.90)
SGU1 AUX  output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0781 at TCP/IP 149.236.99.91)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0345 at TCP/IP 149.236.99.90)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0781 at TCP/IP 149.236.99.91)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0345 at TCP/IP 149.236.99.90)
SGU4 NORM output -> input 3 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0781 at TCP/IP 149.236.99.91)
SGU4 AUX  output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ  W1345097/0345 at TCP/IP 149.236.99.90)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0781 at TCP/IP 149.236.99.91:
- amplifier X-500W uses blanking 4

transmitter 2 = BLAXH2H500/100/250 E 700-900MHZ  W1345097/0345 at TCP/IP 149.236.99.90:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7


