
New TopShim run:

version = topshim 2.0.0
date = 2021-05-10
time = 01:50:04.357
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 2.7 Hz, Target= 0.4 Hz, After= 5.9 Hz
Iteration  2: FWHM Before= 5.9 Hz, Target= 0.4 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.697


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	+3
Z2	+130
Z3	+155
Z4	-2984
Z5	-1332

duration = 34 sec
completed successfully
finished Mon May 10 01:50:35 2021


========================================================================
