
New TopShim run:

version = topshim 2.1.0
date = 2021-12-21
time = 03:21:31.158
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 6.9 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 3: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 4: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 5: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 6: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, non-spinning) = 0.643


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-76
Z2	-32
Z3	+149
Z4	+575
Z5	-613
Z6	-3573
Z7	+3662
Z8	+18884
X	-38
XZ	+7
Y	+7
YZ	-13

duration = 1 min 52 sec
completed successfully
finished Tue Dec 21 03:23:21 2021


========================================================================
