
New TopShim run:

version = topshim 2.0.0
date = 2021-05-07
time = 00:09:30.157
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 3.1 Hz, Target= 0.3 Hz, After= 7.6 Hz
Iteration  2: FWHM Before= 7.6 Hz, Target= 1.0 Hz, After= 0.2 Hz
Iteration  3: FWHM Before= 0.2 Hz, Target= 0.3 Hz, After= 5.9 Hz
Iteration  4: FWHM Before= 5.9 Hz, Target= 0.2 Hz, After= 1.4 Hz
Iteration  5: FWHM Before= 1.4 Hz, Target= 0.2 Hz, After= 1.9 Hz
Iteration  6: FWHM Before= 1.9 Hz, Target= 0.3 Hz, After= 0.7 Hz
Iteration  7: FWHM Before= 0.7 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.769


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+23
Z2	+199
Z3	-343
Z4	-7153
Z5	-895

duration = 1 min 1 sec
completed successfully
finished Fri May  7 00:10:28 2021


========================================================================
