
New TopShim run:

version = topshim 2.0.0
date = 2021-05-09
time = 08:15:04.502
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 3.5 Hz, Target= 0.2 Hz, After= 6.8 Hz
Iteration  2: FWHM Before= 6.8 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  3: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 3.7 Hz
Iteration  4: FWHM Before= 3.7 Hz, Target= 0.3 Hz, After= 0.2 Hz
Iteration  5: FWHM Before= 0.2 Hz, Target= 0.2 Hz, After= 4.7 Hz
Iteration  6: FWHM Before= 4.7 Hz, Target= 0.3 Hz, After= 0.2 Hz
Iteration  7: FWHM Before= 0.2 Hz, Target= 0.2 Hz, After= 3.5 Hz
Iteration  8: FWHM Before= 3.5 Hz, Target= 0.3 Hz, After= 2.8 Hz
Unusually slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, spinning) = 1.71


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+198
Z2	+5
Z3	+374
Z4	-244
Z5	-3448

duration = 1 min 10 sec
completed successfully
finished Sun May  9 08:16:11 2021


========================================================================
