
New TopShim run:

version = topshim 2.0.0
date = 2021-05-09
time = 15:09:18.673
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 2.9 Hz, Target= 0.5 Hz, After= 6.9 Hz
Iteration  2: FWHM Before= 6.9 Hz, Target= 0.5 Hz, After= 0.4 Hz
Iteration  3: FWHM Before= 0.4 Hz, Target= 0.5 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.987


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+13
Z2	+217
Z3	-58
Z4	-7337
Z5	-632

duration = 37 sec
completed successfully
finished Sun May  9 15:09:52 2021


========================================================================
