
New TopShim run:

version = topshim 2.0.0
date = 2021-05-09
time = 22:16:52.260
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 4.5 Hz, Target= 0.5 Hz, After= 0.6 Hz
Iteration  2: FWHM Before= 0.6 Hz, Target= 0.2 Hz, After= 7.3 Hz
Iteration  3: FWHM Before= 7.3 Hz, Target= 0.4 Hz, After= 3.5 Hz
Iteration  4: FWHM Before= 3.5 Hz, Target= 0.5 Hz, After= 0.7 Hz
Iteration  5: FWHM Before= 0.7 Hz, Target= 0.5 Hz, After= 1.4 Hz
Iteration  6: FWHM Before= 1.4 Hz, Target= 0.5 Hz, After= 1.2 Hz
Iteration  7: FWHM Before= 1.2 Hz, Target= 0.2 Hz, After= 7.7 Hz
Iteration  8: FWHM Before= 7.7 Hz, Target= 0.4 Hz, After= 9.3 Hz
Iteration  9: FWHM Before= 9.3 Hz, Target= 0.4 Hz, After= 1.5 Hz
Iteration 10: FWHM Before= 1.5 Hz, Target= 0.5 Hz, After= 0.9 Hz
Iteration 11: FWHM Before= 0.9 Hz, Target= 0.2 Hz, After= 7.3 Hz
Iteration 12: FWHM Before= 7.3 Hz, Target= 0.5 Hz, After=10.3 Hz
Iteration 13: FWHM Before=10.3 Hz, Target= 0.2 Hz, After= 6.9 Hz
Iteration 14: FWHM Before= 6.9 Hz, Target= 0.5 Hz, After= 9.4 Hz
Iteration 15: FWHM Before= 9.4 Hz, Target= 0.2 Hz, After= 6.9 Hz
RMSD between target and map above threshold but maximum number of iterations reached. Halting shimming.

Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, spinning) = 1.21


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	-12
Z2	-3
Z3	-4
Z4	-331
Z5	-933

duration = 1 min 48 sec
completed successfully
finished Sun May  9 22:18:37 2021


========================================================================
