
New TopShim run:

version = topshim 2.0.0
date = 2021-05-07
time = 12:52:15.543
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 4.6 Hz, Target= 0.4 Hz, After= 2.9 Hz
Iteration  2: FWHM Before= 2.9 Hz, Target= 0.3 Hz, After= 0.9 Hz
Iteration  3: FWHM Before= 0.9 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.72


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	-15
Z2	-6
Z3	+99
Z4	-312
Z5	-1411

duration = 36 sec
completed successfully
finished Fri May  7 12:52:49 2021


========================================================================
