
New TopShim run:

version = topshim 2.0.0
date = 2021-05-07
time = 15:59:21.458
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 3.9 Hz, Target= 0.5 Hz, After= 4.5 Hz
Iteration  2: FWHM Before= 4.5 Hz, Target= 0.5 Hz, After= 1.2 Hz
Iteration  3: FWHM Before= 1.2 Hz, Target= 0.5 Hz, After= 0.6 Hz
Iteration  4: FWHM Before= 0.6 Hz, Target= 0.5 Hz, After= 0.5 Hz
Iteration  5: FWHM Before= 0.5 Hz, Target= 0.5 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.591


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	+11
Z2	+47
Z3	+119
Z4	-1348
Z5	-1888

duration = 43 sec
completed successfully
finished Fri May  7 16:00:01 2021


========================================================================
