
New TopShim run:

version = topshim 2.0.0
date = 2021-05-07
time = 16:20:48.859
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 3.8 Hz, Target= 0.7 Hz, After= 0.7 Hz
Iteration  2: FWHM Before= 0.7 Hz, Target= 0.7 Hz, After= 0.7 Hz
Iteration  3: FWHM Before= 0.7 Hz, Target= 0.7 Hz, After= 0.5 Hz
Iteration  4: FWHM Before= 0.5 Hz, Target= 0.7 Hz, After= 0.7 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.802


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-56
Z2	+30
Z3	-20
Z4	-466
Z5	-417

duration = 40 sec
completed successfully
finished Fri May  7 16:21:26 2021


========================================================================
