
New TopShim run:

version = topshim 2.0.0
date = 2021-05-07
time = 17:03:50.481
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 3.8 Hz, Target= 0.2 Hz, After= 5.7 Hz
Iteration  2: FWHM Before= 5.7 Hz, Target= 0.2 Hz, After= 0.2 Hz
Iteration  3: FWHM Before= 0.2 Hz, Target= 0.2 Hz, After= 0.5 Hz
Iteration  4: FWHM Before= 0.5 Hz, Target= 0.2 Hz, After= 0.2 Hz
Iteration  5: FWHM Before= 0.2 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  6: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  7: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.2 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.378


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+77
Z2	+99
Z3	+144
Z4	-2629
Z5	-2708

duration = 54 sec
completed successfully
finished Fri May  7 17:04:41 2021


========================================================================
