
New TopShim run:

version = topshim 2.0.0
date = 2021-05-07
time = 18:20:15.998
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 4.2 Hz, Target= 0.6 Hz, After= 1.4 Hz
Iteration  2: FWHM Before= 1.4 Hz, Target= 0.5 Hz, After= 1.1 Hz
Iteration  3: FWHM Before= 1.1 Hz, Target= 0.6 Hz, After= 0.6 Hz
Iteration  4: FWHM Before= 0.6 Hz, Target= 0.6 Hz, After= 0.7 Hz
Iteration  5: FWHM Before= 0.7 Hz, Target= 0.6 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.78


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-81
Z2	-17
Z3	+4
Z4	+605
Z5	-265

duration = 41 sec
completed successfully
finished Fri May  7 18:20:54 2021


========================================================================
