
New TopShim run:

version = topshim 2.1.0
date = 2021-12-23
time = 10:14:03.595
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.9 Hz, Target= 0.4 Hz, After= 1.0 Hz
Iteration 2: FWHM Before= 1.0 Hz, Target= 0.4 Hz, After= 0.5 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.51


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+56
Z2	+14
Z3	+40
Z4	-39
Z5	-174
Z6	-986
Z7	+437
Z8	+9297
X	+26
XZ	-13
Y	+8
YZ	+15

duration = 1 min 26 sec
completed successfully
finished Thu Dec 23 10:15:28 2021


========================================================================
