
New TopShim run:

version = topshim 2.1.0
date = 2021-12-23
time = 12:46:30.803
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 5.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 1.1 Hz
Iteration 3: FWHM Before= 1.1 Hz, Target= 0.3 Hz, After= 0.9 Hz
Iteration 4: FWHM Before= 0.9 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 5: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 6: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, non-spinning) = 0.4


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+150
Z3	+10
Z4	+174
Z5	-51
Z6	-1212
Z7	-927
Z8	+9913
X	+8
XZ	+7
Y	+42
YZ	+2

duration = 1 min 39 sec
completed successfully
finished Thu Dec 23 12:48:08 2021


========================================================================
