
New TopShim run:

version = topshim 2.1.0
date = 2021-12-23
time = 16:22:55.184
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 4.9 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 2: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.2 Hz
Iteration 3: FWHM Before= 0.2 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.575


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+131
Z2	-34
Z3	+6
Z4	+783
Z5	-101
Z6	-4540
Z7	-250
Z8	+20428
X	+14
XZ	-6
Y	+8
YZ	+8

duration = 1 min 22 sec
completed successfully
finished Thu Dec 23 16:24:15 2021


========================================================================
