
New TopShim run:

version = topshim 2.0.0
date = 2021-05-08
time = 22:33:30.647
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 4.5 Hz, Target= 0.2 Hz, After= 4.0 Hz
Iteration  2: FWHM Before= 4.0 Hz, Target= 0.2 Hz, After= 0.8 Hz
Iteration  3: FWHM Before= 0.8 Hz, Target= 0.2 Hz, After= 0.4 Hz
Iteration  4: FWHM Before= 0.4 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  5: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.2 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.814


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	+9
Z2	+76
Z3	+173
Z4	-2023
Z5	-1703

duration = 44 sec
completed successfully
finished Sat May  8 22:34:13 2021


========================================================================
