
New TopShim run:

version = topshim 2.0.0
date = 2021-05-11
time = 22:41:14.795
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 1.1 Hz, Target= 0.3 Hz, After= 4.1 Hz
Iteration  2: FWHM Before= 4.1 Hz, Target= 0.7 Hz, After= 2.6 Hz
Iteration  3: FWHM Before= 2.6 Hz, Target= 0.7 Hz, After= 0.7 Hz
Iteration  4: FWHM Before= 0.7 Hz, Target= 0.7 Hz, After= 0.7 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.819


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-56
Z2	+24
Z3	-132
Z4	-532
Z5	+943

duration = 43 sec
completed successfully
finished Tue May 11 22:41:54 2021


========================================================================
