
New TopShim run:

version = topshim 2.0.0
date = 2021-05-12
time = 00:10:39.947
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 1.0 Hz, Target= 0.5 Hz, After= 1.1 Hz
Iteration  2: FWHM Before= 1.1 Hz, Target= 0.3 Hz, After= 2.4 Hz
Iteration  3: FWHM Before= 2.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.566


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+57
Z2	+1
Z3	+253
Z4	+91
Z5	-1604

duration = 40 sec
completed successfully
finished Wed May 12 00:11:17 2021


========================================================================
