
New TopShim run:

version = topshim 2.0.0
date = 2021-05-12
time = 05:09:26.504
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 1.6 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration  2: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.564


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+34
Z2	-26
Z3	+49
Z4	+480
Z5	-984

duration = 34 sec
completed successfully
finished Wed May 12 05:09:57 2021


========================================================================
