
New TopShim run:

version = topshim 2.0.0
date = 2021-05-14
time = 14:45:00.095
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 0.6 Hz, Target= 0.2 Hz, After= 0.2 Hz
Iteration  2: FWHM Before= 0.2 Hz, Target= 0.2 Hz, After= 0.6 Hz
Iteration  3: FWHM Before= 0.6 Hz, Target= 0.2 Hz, After= 0.6 Hz
Iteration  4: FWHM Before= 0.6 Hz, Target= 0.2 Hz, After= 0.2 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.783


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-90
Z2	-120
Z3	-1196
Z4	-7233
Z5	-586

duration = 42 sec
completed successfully
finished Fri May 14 14:45:39 2021


========================================================================
