
New TopShim run:

version = topshim 2.0.0
date = 2021-05-14
time = 19:27:00.850
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 0.5 Hz, Target= 0.3 Hz, After=15.6 Hz
Iteration  2: FWHM Before=15.6 Hz, Target= 0.2 Hz, After= 0.6 Hz
Iteration  3: FWHM Before= 0.6 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  4: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  5: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration  6: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.318


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	+340
Z2	-105
Z3	-1063
Z4	-8587
Z5	-6622

duration = 51 sec
completed successfully
finished Fri May 14 19:27:49 2021


========================================================================
