
New TopShim run:

version = topshim 2.0.0
date = 2021-05-14
time = 23:31:17.040
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 0.9 Hz, Target= 0.5 Hz, After= 1.1 Hz
Iteration  2: FWHM Before= 1.1 Hz, Target= 0.3 Hz, After= 0.9 Hz
Iteration  3: FWHM Before= 0.9 Hz, Target= 0.3 Hz, After= 0.5 Hz
Iteration  4: FWHM Before= 0.5 Hz, Target= 0.5 Hz, After= 0.8 Hz
Iteration  5: FWHM Before= 0.8 Hz, Target= 0.2 Hz, After= 1.9 Hz
Iteration  6: FWHM Before= 1.9 Hz, Target= 0.5 Hz, After= 1.8 Hz
Diverging behaviour detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, spinning) = 0.659


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-4
Z2	+14
Z3	+152
Z4	+165
Z5	-498

duration = 53 sec
completed successfully
finished Fri May 14 23:32:07 2021


========================================================================
