
New TopShim run:

version = topshim 2.0.0
date = 2021-05-15
time = 01:50:00.428
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 1.2 Hz, Target= 0.4 Hz, After= 2.2 Hz
Iteration  2: FWHM Before= 2.2 Hz, Target= 0.3 Hz, After= 0.7 Hz
Iteration  3: FWHM Before= 0.7 Hz, Target= 0.4 Hz, After= 1.1 Hz
Iteration  4: FWHM Before= 1.1 Hz, Target= 0.3 Hz, After= 0.6 Hz
Iteration  5: FWHM Before= 0.6 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration  6: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.7 Hz
Iteration  7: FWHM Before= 0.7 Hz, Target= 0.3 Hz, After= 0.5 Hz
Slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, spinning) = 0.77


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	+96
Z2	+16
Z3	+81
Z4	-474
Z5	-1815

duration = 53 sec
completed successfully
finished Sat May 15 01:50:51 2021


========================================================================
