
New TopShim run:

version = topshim 2.0.0
date = 2021-05-15
time = 02:44:58.956
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 1.7 Hz, Target= 0.9 Hz, After= 0.9 Hz
Iteration  2: FWHM Before= 0.9 Hz, Target= 0.9 Hz, After= 0.8 Hz
Iteration  3: FWHM Before= 0.8 Hz, Target= 0.6 Hz, After= 0.4 Hz
Iteration  4: FWHM Before= 0.4 Hz, Target= 0.8 Hz, After= 3.9 Hz
Iteration  5: FWHM Before= 3.9 Hz, Target= 0.9 Hz, After= 2.8 Hz
Iteration  6: FWHM Before= 2.8 Hz, Target= 0.7 Hz, After= 0.4 Hz
Iteration  7: FWHM Before= 0.4 Hz, Target= 0.9 Hz, After= 1.8 Hz
Iteration  8: FWHM Before= 1.8 Hz, Target= 0.9 Hz, After= 2.6 Hz
Iteration  9: FWHM Before= 2.6 Hz, Target= 0.9 Hz, After= 2.1 Hz
Iteration 10: FWHM Before= 2.1 Hz, Target= 0.9 Hz, After= 0.8 Hz
Iteration 11: FWHM Before= 0.8 Hz, Target= 0.9 Hz, After= 1.0 Hz
Iteration 12: FWHM Before= 1.0 Hz, Target= 0.9 Hz, After= 0.8 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.95


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-65
Z2	+54
Z3	-178
Z4	-762
Z5	+1096

duration = 1 min 21 sec
completed successfully
finished Sat May 15 02:46:17 2021


========================================================================
