
New TopShim run:

version = topshim 2.1.0
date = 2021-12-21
time = 06:21:17.229
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.8 Hz, Target= 0.5 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.5 Hz, After= 0.4 Hz
Iteration 3: FWHM Before= 0.4 Hz, Target= 0.5 Hz, After= 0.5 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.628


Performing tune after shimming
tune lock level increase = 1.1

shim changes: 
Z	+100
Z2	-8
Z3	+12
Z4	+401
Z5	-94
Z6	-3138
Z7	-100
Z8	+16674
X	+26
XZ	+33
Y	+1
YZ	+16

duration = 1 min 31 sec
completed successfully
finished Tue Dec 21 06:22:46 2021


========================================================================
