
New TopShim run:

version = topshim 2.1.0
date = 2021-12-21
time = 13:23:50.976
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 4.5 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.3 Hz
Iteration 3: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 4: FWHM Before= 0.3 Hz, Target= 0.2 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.51


Performing tune after shimming
tune lock level increase = 1.1

shim changes: 
Z	-471
Z2	-80
Z3	+333
Z4	+1044
Z5	-1492
Z6	-3217
Z7	+10886
Z8	+8658
X	+26
Y	+54
YZ	+7

duration = 1 min 38 sec
completed successfully
finished Tue Dec 21 13:25:27 2021


========================================================================
