
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 06:14:36.800
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 4.5 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 2: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 3: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 4: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.46


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+129
Z2	+2
Z3	+26
Z4	+154
Z5	-77
Z6	-1529
Z7	-624
Z8	+10341
X	+8
XZ	+8
Y	+8
YZ	+8

duration = 1 min 23 sec
completed successfully
finished Wed Dec 22 06:15:58 2021


========================================================================
