
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 06:39:21.952
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 0.8 Hz, Target= 0.2 Hz, After= 0.5 Hz
Iteration 2: FWHM Before= 0.5 Hz, Target= 0.2 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.427


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+201
Z2	+17
Z3	-47
Z4	-169
Z5	+140
Z6	-66
Z7	-1765
Z8	+7824
X	-59
XZ	+8
Y	-2
YZ	-22

duration = 1 min 35 sec
completed successfully
finished Wed Dec 22 06:40:55 2021


========================================================================
