
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 08:06:52.805
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 4.3 Hz, Target= 0.4 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.7 Hz
Iteration 3: FWHM Before= 0.7 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 4: FWHM Before= 0.3 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 5: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.2 Hz
Iteration 6: FWHM Before= 0.2 Hz, Target= 0.3 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.546


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+127
Z2	-3
Z3	+9
Z4	+323
Z5	-64
Z6	-2193
Z7	-531
Z8	+12205
X	+8
XZ	+33
Y	+21
YZ	+6

duration = 1 min 38 sec
completed successfully
finished Wed Dec 22 08:08:29 2021


========================================================================
