
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 12:58:51.913
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.3 Hz, Target= 0.5 Hz, After= 0.7 Hz
Iteration 2: FWHM Before= 0.7 Hz, Target= 0.4 Hz, After= 0.2 Hz
Iteration 3: FWHM Before= 0.2 Hz, Target= 0.5 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.524


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-42
Z2	-24
Z3	+88
Z4	+406
Z5	-441
Z6	-3060
Z7	+2907
Z8	+18898
X	+10
XZ	+38
Y	-13
YZ	-37

duration = 1 min 33 sec
completed successfully
finished Wed Dec 22 13:00:23 2021


========================================================================
