
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 14:26:04.567
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.6 Hz, Target= 0.5 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.5 Hz, After= 1.3 Hz
Iteration 3: FWHM Before= 1.3 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 4: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 5: FWHM Before= 0.4 Hz, Target= 0.5 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.519


Performing tune after shimming
tune lock level increase = 1.1

shim changes: 
Z	+87
Z2	-22
Z3	+14
Z4	+580
Z5	-162
Z6	-3717
Z7	+611
Z8	+18322
X	+8
XZ	+3
Y	+8
YZ	+8

duration = 1 min 26 sec
completed successfully
finished Wed Dec 22 14:27:29 2021


========================================================================
