
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 18:12:13.046
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 5.1 Hz, Target= 0.4 Hz, After= 0.9 Hz
Iteration 2: FWHM Before= 0.9 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 3: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.6 Hz
Iteration 4: FWHM Before= 0.6 Hz, Target= 0.4 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.487


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+60
Z2	-15
Z3	+62
Z4	+351
Z5	-255
Z6	-2304
Z7	+803
Z8	+12558
X	+8
XZ	-24
Y	+10
YZ	-86

duration = 1 min 41 sec
completed successfully
finished Wed Dec 22 18:13:53 2021


========================================================================
