
New TopShim run:

version = topshim 2.1.0
date = 2021-12-22
time = 18:49:47.037
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 5.3 Hz, Target= 0.4 Hz, After= 0.7 Hz
Iteration 2: FWHM Before= 0.7 Hz, Target= 0.4 Hz, After= 0.3 Hz
Iteration 3: FWHM Before= 0.3 Hz, Target= 0.4 Hz, After= 0.3 Hz
Iteration 4: FWHM Before= 0.3 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 5: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 6: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.3 Hz
Slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, non-spinning) = 0.545


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+81
Z2	+5
Z3	+42
Z4	+34
Z5	-141
Z6	-756
Z7	+4
Z8	+7281
X	-12
XZ	+14
Y	+17
YZ	+16

duration = 1 min 42 sec
completed successfully
finished Wed Dec 22 18:51:27 2021


========================================================================
