
New TopShim run:

version = topshim 2.1.0
date = 2021-12-23
time = 00:31:49.472
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 5.1 Hz, Target= 0.3 Hz, After= 0.6 Hz
Iteration 2: FWHM Before= 0.6 Hz, Target= 0.4 Hz, After= 1.0 Hz
Iteration 3: FWHM Before= 1.0 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 4: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.7 Hz
Iteration 5: FWHM Before= 0.7 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 6: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.4 Hz
Slow convergence detected. Shimming was aborted.
Using the best result as the final shim state.

Lineshape quality factor (1D spectrum, non-spinning) = 0.426


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+180
Z2	-15
Z3	-6
Z4	+471
Z5	+7
Z6	-3053
Z7	-1305
Z8	+15514
X	-43
Y	+3
YZ	+10

duration = 1 min 52 sec
completed successfully
finished Thu Dec 23 00:33:40 2021


========================================================================
