EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
T_NAME		Date_
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 50000000
		REL	"Date_=itodate(DATE)"
		INV_REL	"DATE=datetoi(Date_,DATE)"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		Time
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"Time=itotime(DATE)"
		INV_REL	"DATE=timetoi(Time,DATE)"
		FORMAT	"%14.2f"
		TEXT	" "
END
NAME		INSTRUM
		TEXT	" "
END
NAME		PROBHD
		FORMAT	"%14.14s"
		TEXT	" "
END
NAME		PULPROG
		TEXT	" "
END
NAME		TD
		TEXT	" "
END
NAME		SOLVENT
		TEXT	" "
END
NAME		NS
		TEXT	" "
END
NAME		DS
		TEXT	" "
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e8
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.3f Hz"
		TEXT	" "
END
T_NAME          FIDRES
                TYPE    R32
                CLASS   ACQU
                SUBRANGE 0.0 100000
                REL     "FIDRES=SW*SFO1/TD"
                INV_REL "TD = nextpow(SW*SFO1/FIDRES)"
		UNIT	"Hz"
		FORMAT	"%14.6f Hz"
		TEXT	" "
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
		TEXT	" "
END
NAME		RG
		TEXT	" "
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3lf usec"
		TEXT	" "
END
NAME		DE
		FORMAT	"%14.2f usec"
		TEXT	" "
END
NAME		TE
		FORMAT	"%14.1f K"
		TEXT	" "
END
T_NAME		d0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d0=3u"
		INV_REL	"D[0]=d0"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		d11
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d11=100m"
		INV_REL	"D[0]=d11"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d14
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d14=40u"
		INV_REL	"D[0]=d14"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		d16
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d16=300u"
		INV_REL	"D[0]=d16"
		UNIT	"sec"
		TEXT	" "
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		IN0
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"IN0=IN[0]"
		INV_REL	"IN[0]=IN0"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
		TEXT	" "
END
T_NAME		L1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"L1=L[1]"
		INV_REL	"L[1]=L1"
		FORMAT	"%14.0f"
		TEXT	" "
END
T_NAME		L4
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1000000
		REL	"L4=L[4]"
		INV_REL	"L[4]=L4"
		FORMAT	"%14.0f"
		TEXT	" "
END
HEADER		"============ CHANNEL f1 ============="
NAME		NUC1
		TEXT	" "
END
T_NAME		P1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P1=P[1]"
		INV_REL	"P[1]=P1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P2=P[2]"
		INV_REL	"P[2]=P2"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P14=P[14]"
		INV_REL	"P[14]=P14"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		P15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P15=P[15]"
		INV_REL	"P[15]=P15"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
		TEXT	" "
END
T_NAME		PL1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"PL1=PL[1]"
		INV_REL	"PL[1]=PL1"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
T_NAME		PL11
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"PL11=PL[11]"
		INV_REL	"PL[11]=PL11"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	" "
END
T_NAME		SP14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"SP14=SP[14]"
		INV_REL	"SP[14]=SP14"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
T_NAME		SP15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 120
		REL	"SP15=SP[15]"
		INV_REL	"SP[15]=SP15"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
		TEXT	" "
END
NAME		SPNAM14
		TEXT	" "
END
NAME		SPNAM15
		TEXT	" "
END
T_NAME		SPOFF14
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1000000 1000000
		REL	"SPOFF14=SPOFFS[14]"
		INV_REL	"SPOFFS[14]=SPOFF14"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
T_NAME		SPOFF15
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1000000 1000000
		REL	"SPOFF15=SPOFFS[15]"
		INV_REL	"SPOFFS[15]=SPOFF15"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	" "
END
HEADER		"============ GRADIENT CHANNEL ========"
T_NAME		GPX5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX5=GPX[5]"
		INV_REL	"GPX[5]=GPX5"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX6
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX6=GPX[6]"
		INV_REL	"GPX[6]=GPX6"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX7
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX7=GPX[7]"
		INV_REL	"GPX[7]=GPX7"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPX8
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPX8=GPX[8]"
		INV_REL	"GPX[8]=GPX8"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY5=GPY[5]"
		INV_REL	"GPY[5]=GPY5"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY6
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY6=GPY[6]"
		INV_REL	"GPY[6]=GPY6"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY7
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY7=GPY[7]"
		INV_REL	"GPY[7]=GPY7"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPY8
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPY8=GPY[8]"
		INV_REL	"GPY[8]=GPY8"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ5
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ5=GPZ[5]"
		INV_REL	"GPZ[5]=GPZ5"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ6
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ6=GPZ[6]"
		INV_REL	"GPZ[6]=GPZ6"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ7
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ7=GPZ[7]"
		INV_REL	"GPZ[7]=GPZ7"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
T_NAME		GPZ8
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ8=GPZ[8]"
		INV_REL	"GPZ[8]=GPZ8"
		UNIT	"%"
		FORMAT	"%14.2f %"
		TEXT	" "
END
