CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2.5/conf/instr/spect/uxnmr.info
Date         : Fri Feb 20 15:28:09 2015
Release      : TOPSPIN Version 3.2-pl5
Installed in : /opt/topspin3.2.5
Host         : kerry.nmrfam.wisc.edu
OS           : CentOS release 5.5 (Final)
CPU          : Intel(R) Core(TM)2 Duo CPU E7200 @ 2.53GHz (2 cores at 2533 MHz)
User         : bmrbmb (Bmrb Metabolomics,,,,,,BMRB)
Description  : Avance III 500
Location     : 
System       : Avance III NMR spectrometer
1H-frequency : 499.84 MHz
Order Number : 
Configured in: /opt/topspin3.2.5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/01517 ECL 05.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2
DRU: AQS DRU-E Z102520/01518 ECL 05.00
- TCP/IP address = 149.236.99.88
- Firmware Version = 130419

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.4 REC-1  AQS RXAD600 Z102117/682 ECL 04.04
     3   0x34 0xc0   0x1        X  2.2 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.6 SGU-1  AQS SGU/2 600 Z103081/01332 ECL 02.06 FPGA-Vs=AF
     6   0x11 0x42   0x4    AW  R  4.4 REC-2  AQS RXAD600 Z102117/683 ECL 04.04
     7   0x25 0x19   0x8    AE  S  2.6 SGU-2  AQS SGU/2 600 Z103081/01333 ECL 02.06 FPGA-Vs=AF
     8   0x26 0x19   0x8    AE  S  2.6 SGU-3  AQS SGU/2 600 Z103081/01321 ECL 02.06 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0389 W1345096/0389 ECL 2:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0389 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0629 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00749 ECL 03
- QNP-Accessory  : 1 X-input and 1 H-input
BLA_W1345092_0272 W1345092/0272 ECL 1:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0272 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0819 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00730 ECL 03
LTRX Z109889/00009 ECL 00.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00009 ECL 00.00

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20140110
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00009 ECL 00.00
- Lock: on L-TRX board

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty04
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - SampleJet: at TCP/IP address 149.236.99.55


Cryo Controller CRCO: device connected to 149.236.99.254:/dev/tty01

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003461, SN=00675 from 20090123
    Module  2 : XBB19F 2HS
                 PN=Z003505, SN=00752 from 20081215
    Module  3 : 2H
                 PN=Z003472, SN=00705 from 20090117
    Module  4 : 15N
                 PN=Z003529, SN=00162 from 20090109
    Module  5 : 13C
                 PN=Z003523, SN=00187 from 20090204


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0272 at TCP/IP 149.236.99.249)
SGU3 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250) amplifier X-300W uses blanking 1
transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250) amplifier 2H-150W needs no blanking
transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0272 at TCP/IP 149.236.99.249) amplifier X-300W uses blanking 4
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 500 Z109889/00009 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250 amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250 amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
BLAXH2H300/100/150 E 200-600MHZ W1345096/0389 at TCP/IP 149.236.99.250 amplifier 2H-150W can be routed to switchbox output 5 (unknown)

