CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl7/conf/instr/spect/uxnmr.info
Date         : Tue Jul 30 09:58:29 2019
Release      : TopSpin 3.5 pl 7
Installed in : /opt/topspin3.5pl7
Host         : kerry.nmrfam.wisc.edu
OS           : CentOS release 5.5 (Final)
CPU          : Intel(R) Core(TM)2 Duo CPU E7200 @ 2.53GHz (2 cores at 2533 MHz)
User         : paulo (Paulo Falco Cobra)
System       : Avance III 500 NMR spectrometer
1H-frequency : 499.84 MHz
Description  : Avance III 500 Kerry
Configured in: kerry.nmrfam.wisc.edu:/opt/topspin3.5pl7/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01517 ECL 05.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2
DRU2: AQS DRU-E Z102520/01518 ECL 05.00
- TCP/IP address = 149.236.99.88
- Firmware Version = 170619

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.4 REC-1  AQS RXAD600 Z102117/682 ECL 04.04
     3   0x34 0xc0   0x1        X  2.2 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.6 SGU-1  AQS SGU/2 600 Z103081/01332 ECL 02.06 FPGA-Vs=AF
     6   0x11 0x42   0x4    AW  R  4.4 REC-2  AQS RXAD600 Z102117/683 ECL 04.04
     7   0x25 0x19   0x8    AE  S  2.6 SGU-2  AQS SGU/2 600 Z103081/01333 ECL 02.06 FPGA-Vs=AF
     8   0x26 0x19   0x8    AE  S  2.6 SGU-3  AQS SGU/2 600 Z103081/01321 ECL 02.06 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0389 W1345096/0389 ECL 2:
- TCP/IP address = 149.236.99.250
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0389 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0629 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00749 ECL 03
- QNP-Accessory  : 1 X-input and 1 H-input
BLA_W1345092_0272 W1345092/0272 ECL 1:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0272 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0819 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/00730 ECL 03
LTRX Z109889/00009 ECL 00.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00009 ECL 00.00

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20170712
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 500: Z109889/00009 ECL 00.00
- Lock: on L-TRX board

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty04
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.254:/dev/tty01

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty05

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 149.236.99.55

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003461, SN=00675 from 20090123
    Module  2 : XBB19F 2HS
                PN=Z003505, SN=00752 from 20081215
    Module  3 : 2H
                PN=Z003472, SN=00705 from 20090117
    Module  4 : 15N
                PN=Z003529, SN=00162 from 20090109
    Module  5 : 13C
                PN=Z003523, SN=00187 from 20090204



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0389 at TCP/IP 149.236.99.250)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0389 at TCP/IP 149.236.99.250)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0272 at TCP/IP 149.236.99.249)
SGU3 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0389 at TCP/IP 149.236.99.250)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0389 at TCP/IP 149.236.99.250:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking

transmitter 2 = BLAX300 E 6-365MHZ INR W1345092/0272 at TCP/IP 149.236.99.249:
- amplifier X-300W uses blanking 4

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 500 Z109889/00009 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ INR W1345096/0389 at TCP/IP 149.236.99.250:
- amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
- amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
- amplifier 2H-150W can be routed to switchbox output 5 (unknown)


