EDIT_PAR COMMAND FILE

DI_MODE         LONG
ED_ENTRY        ACQU
ORDER           FILE


HEADER		"F2 - Acquisition Parameters"
NAME		PULPROG
END
NAME		TD
END
NAME		NS
END
NAME		DS
END
T_NAME		SWH
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"SWH=SW*SFO1"
		INV_REL "SW=SWH/SFO1"
		UNIT	"Hz"
		FORMAT	"%14.2f Hz"
		TEXT	"sweep width in Hz"
END
T_NAME          AQ
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"AQ=aqcalc(SW,SFO1,TD,DIGTYP)"
		INV_REL	"TD=tdcalc(SW,SFO1,1.0e6*AQ,DIGTYP)"
		UNIT	"sec"
		FORMAT	"%14.7f sec"
                TEXT	"acquisition time"
END
NAME		RG
END
T_NAME          DW
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"DW=1/(2*SW*SFO1)"
		INV_REL	"SW=1000000/(2*(0.005+DW)*SFO1)"
		UNIT	"usec"
		FORMAT	"%14.3f usec"
		TEXT	"dwell time "
END
NAME		DE
		FORMAT	"%14.2f usec"
END
T_NAME		CNST13
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -1e38 1e38
		REL	"CNST13=CNST[13]"
		INV_REL	"CNST[13]=CNST13"
		FORMAT	"%14.7f"
TEXT		"= J(XH) long range"
END
T_NAME		d0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d0=3u"
		INV_REL	"D[0]=d0"
		UNIT	"sec"
		TEXT	"d0=3u"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D1=D[1]"
		INV_REL	"D[1]=D1"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
TEXT		"relaxation delay; 1-5 * T1"
END
T_NAME		d6
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"d6=1s/(cnst13*2)"
		INV_REL	"D[0]=d6"
		UNIT	"sec"
		TEXT	"d6=1s/(cnst13*2)"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		D16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"D16=D[16]"
		INV_REL	"D[16]=D16"
		UNIT	"sec"
		FORMAT	"%14.8f sec"
TEXT		"delay for homospoil/gradient recovery"
END
T_NAME		in0
		TYPE	R32
		SUBRANGE 0.0 1e8
		CLASS	ACQU
		REL	"in0=inf1/2"
		INV_REL	"D[0]=in0"
		UNIT	"sec"
		TEXT	"in0=inf1/2"
		FORMAT	"%14.8f sec"
		NONEDIT
END
T_NAME		INF1
		TYPE	R64
		CLASS	ACQU
		SUBRANGE 0.0 1e38
		REL	"INF1=INF[1]"
		INV_REL	"INF[1]=INF1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"1/SW(X) = 2 * DW(X)"
		NONEDIT
END
HEADER		"======== CHANNEL f1 ========"
NAME		NUC1
		NONEDIT
		TEXT	"nucleus for channel 1"
END
T_NAME		P1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P1=P[1]"
		INV_REL	"P[1]=P1"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"f1 channel -  90 degree high power pulse"
END
T_NAME		p2
		TYPE	R32
		SUBRANGE -1e38 1e38
		CLASS	ACQU
		REL	"p2=p1*2"
		INV_REL	"D[0]=p2"
		UNIT	"usec"
		TEXT	"p2=p1*2"
		FORMAT	"%14.2f usec"
		NONEDIT
END
T_NAME		PL1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL1=PL[1]"
		INV_REL	"PL[1]=PL1"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
TEXT		"f1 channel - power level for pulse (default)"
END
T_NAME		PL1W
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL1W=106*pow(10.0,(-6-PL[1])/10.0)"
		INV_REL	"PL[1]=-6-4.3425*log(PL1W/106)"
		UNIT	"no"
		FORMAT	"%14.8f W"
TEXT		"f1 channel - power level for pulse (default)"
END
NAME		SFO1
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of observe channel"
END
HEADER		"======== CHANNEL f2 ========"
NAME		NUC2
		NONEDIT
		TEXT	"nucleus for channel 2"
END
T_NAME		P3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P3=P[3]"
		INV_REL	"P[3]=P3"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"f2 channel -  90 degree high power pulse"
END
T_NAME		PL2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL2=PL[2]"
		INV_REL	"PL[2]=PL2"
		UNIT	"dB"
		FORMAT	"%14.2f dB"
TEXT		"f2 channel - power level for pulse (default)"
END
T_NAME		PL2W
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -6.0 1e38
		REL	"PL2W=288*pow(10.0,(-6-PL[2])/10.0)"
		INV_REL	"PL[2]=-6-4.3425*log(PL2W/288)"
		UNIT	"no"
		FORMAT	"%14.8f W"
TEXT		"f2 channel - power level for pulse (default)"
END
NAME		SFO2
		FORMAT	"%14.7f MHz"
		TEXT	"frequency of observe channel"
END
HEADER		"====== GRADIENT CHANNEL ====="
NAME		GPNAM1
TEXT		"SINE.100"
END
NAME		GPNAM2
TEXT		"SINE.100"
END
NAME		GPNAM3
TEXT		"SINE.100"
END
T_NAME		GPZ1
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ1=GPZ[1]"
		INV_REL	"GPZ[1]=GPZ1"
		UNIT	"%"
		FORMAT	"%14.2f %"
TEXT		"50% for C-13, 70% for N-15"
END
T_NAME		GPZ2
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ2=GPZ[2]"
		INV_REL	"GPZ[2]=GPZ2"
		UNIT	"%"
		FORMAT	"%14.2f %"
TEXT		"30%"
END
T_NAME		GPZ3
		TYPE	R32
		CLASS	ACQU
		SUBRANGE -100.0 100.0
		REL	"GPZ3=GPZ[3]"
		INV_REL	"GPZ[3]=GPZ3"
		UNIT	"%"
		FORMAT	"%14.2f %"
TEXT		"40.1% for C-13, 50.1% for N-15"
END
T_NAME		P16
		TYPE	R32
		CLASS	ACQU
		SUBRANGE 0.0 1.0e10
		REL	"P16=P[16]"
		INV_REL	"P[16]=P16"
		UNIT	"usec"
		FORMAT	"%14.2f usec"
TEXT		"homospoil/gradient pulse"
END
