NMRbot_cq_dl_gl_pch_SampleReport.20131118_1616.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## NMRbot version 20131115 ##

## Initiated - 20131118_1616 ##

- info:
  cq_dl_gl_pch in CDCl3 at position 201
  foldername => cq_dl_gl_pch.CDCl3.201.20131118
  Exps => ZGCPPR,metabTOCSY,C13CPD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 201 - passed
-   sample solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 22.6
- creating exp 2 with metabTOCSY parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 64
- creating exp 3 with C13CPD parameters - passed
-   prosol parameters loaded
-   NS changed to 2048
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters - passed
-   prosol parameters loaded
-   NS changed to 512
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters - passed
-   prosol parameters loaded
-   NS changed to 512
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters - passed
-   prosol parameters loaded
-   NS changed to 4
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters - passed
-   prosol parameters loaded
-   NS changed to 4
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND parameters - passed
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 32
- creating exp 10 with HSQC_TOCSY_ADIA parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
-     dims %s- F1 1H, SW 16.0307
- start 20131118_1626
- end   20131118_1627 - passed
-   1H adaptive offset determined = 4.7498
-   1H adaptive SW determined = 8.9723
# Exp 2 - metabTOCSY (mlevph)
-     dims %s- F1 1H, SW 10.2073; F2 1H, SW 10.2073
- start 20131118_1627
- end   20131118_1904 - passed
# Exp 3 - C13CPD (zgpg30)
-     dims %s- F1 13C, SW 236.7742
- start 20131118_1904
- end   20131118_2053 - passed
# Exp 4 - C13DEPT90 (dept90)
-     dims %s- F1 13C, SW 236.7742
- start 20131118_2053
- end   20131118_2120 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
-     dims %s- F1 13C, SW 236.7742
- start 20131118_2120
- end   20131118_2147 - passed
-   13C adaptive offset determined = 93.7494
-   13C adaptive SW determined = 169.6835
# Exp 6 - HSQCETGP (hsqcetgp)
-     dims %s- F1 13C, SW 165.6393; F2 1H, SW 13.3375
- start 20131118_2147
- end   20131118_2215 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-     dims %s- F1 13C, SW 165.6393; F2 1H, SW 13.3375
-   F1 SW changed to 169.6835
-   F2 SW changed to 8.9723
-   F1 1H offset changed to 4.7498
-   F2 13C offset changed to 93.7494
- start 20131118_2215
- end   20131118_2243 - passed
# Exp 8 - HMBCETGPL3ND (hmbcetgpl3nd)
-     dims %s- F1 13C, SW 221.8327; F2 1H, SW 12.0230
- start 20131118_2243
- end   20131119_0007 - passed
# Exp 9 - COSY45SW (cosyqf45)
-     dims %s- F1 1H, SW 10.3125; F2 1H, SW 10.3125
- start 20131119_0007
- end   20131119_0123 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
-     dims %s- F1 13C, SW 165.6580; F2 1H, SW 11.9655
- start 20131119_0123
- end   20131119_0358 - passed

## cq_dl_gl_pch Experiment Set Ended - 20131119_0358 ##

