NMRbot_cq_14162_SampleReport.20140115_1333.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## NMRbot version 20140114 ##

## Initiated - 20140115_1333 ##

- info:
  cq_14162 in CDCl3 at position 205
  foldername => cq_14162.CDCl3.205.20140114
  Exps => ZGCPPR,metabTOCSY,C13CPD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 205 - passed
-   sample solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 64
- creating exp 2 with metabTOCSY parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 3 with C13CPD parameters - passed
-   prosol parameters loaded
-   NS changed to 2048
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters - passed
-   prosol parameters loaded
-   NS changed to 512
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters - passed
-   prosol parameters loaded
-   NS changed to 512
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters - passed
-   prosol parameters loaded
-   NS changed to 4
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters - passed
-   prosol parameters loaded
-   NS changed to 4
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND parameters - passed
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 10 with HSQC_TOCSY_ADIA parameters - passed
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
-     dims 1- F1 1H, SW 16.0307
- start 20140115_1343
- end   20140115_1345 - passed
-   1H adaptive offset determined = 4.7498
-   1H adaptive SW determined = 10.2271
# Exp 2 - metabTOCSY (mlevph)
-     dims 2- F1 1H, SW 10.2073; F2 1H, SW 10.2073
- start 20140115_1345
- end   20140115_1622 - passed
# Exp 3 - C13CPD (zgpg30)
-     dims 1- F1 13C, SW 236.7742
- start 20140115_1622
- end   20140115_1810 - passed
# Exp 4 - C13DEPT90 (dept90)
-     dims 1- F1 13C, SW 236.7742
- start 20140115_1810
- end   20140115_1837 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
-     dims 1- F1 13C, SW 236.7742
- start 20140115_1837
- end   20140115_1905 - passed
-   13C adaptive offset determined = 45.7036
-   13C adaptive SW determined = 73.0739
# Exp 6 - HSQCETGP (hsqcetgp)
-     dims 2- F1 13C, SW 165.6393; F2 1H, SW 13.3375
- start 20140115_1905
- end   20140115_1932 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-     dims 2- F1 13C, SW 165.6393; F2 1H, SW 13.3375
-   F1 SW changed to 73.0739
-   F2 SW changed to 10.2271
-   F1 1H offset changed to 4.7498
-   F2 13C offset changed to 45.7036
- start 20140115_1933
- end   20140115_2001 - passed
# Exp 8 - HMBCETGPL3ND (hmbcetgpl3nd)
-     dims 2- F1 13C, SW 221.8327; F2 1H, SW 12.0230
- start 20140115_2001
- end   20140115_2124 - passed
# Exp 9 - COSY45SW (cosyqf45)
-     dims 2- F1 1H, SW 10.3125; F2 1H, SW 10.3125
- start 20140115_2124
- end   20140115_2240 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
-     dims 2- F1 13C, SW 165.6580; F2 1H, SW 11.9655
- start 20140115_2240
- end   20140116_0116 - passed

## cq_14162 Experiment Set Ended - 20140116_0116 ##

