NMRbot_cq_01158_SampleReport.20160826_2055.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## NMRbot version 20140226 ##

## Initiated - 20160826_2055 ##

- info:
  cq_01158 in D2O at position 202
  foldername => cq_01158.D2O.202.20160826
  Exps => ZGCPPR,metabTOCSY,C13CPD_MMCD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 202 - passed
- D2O solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
-   determined 1H offset = 0.7888
- creating exp 1 with ZGCPPR parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 2 with metabTOCSY parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 3 with C13CPD_MMCD parameters
-   prosol parameters loaded
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters
-   prosol parameters loaded
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters
-   prosol parameters loaded
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 10 with HSQC_TOCSY_ADIA parameters
-   prosol parameters loaded
-   1H offset changed to 0.7888
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
- dims 1- F1 1H, SW 16.03
- start 20160826_2109
- end   20160826_2110 - passed
-   1H adaptive offset determined = 0.7888
-   1H adaptive SW determined = 9.1976
# Exp 2 - metabTOCSY (mlevph)
- dims 2- F1 1H, SW 10.21; F2 1H, SW 10.21
- start 20160826_2110
- end   20160826_2229 - passed
# Exp 3 - C13CPD_MMCD (zgpg30)
- dims 1- F1 13C, SW 248.61
- start 20160826_2229
- end   20160826_2323 - passed
# Exp 4 - C13DEPT90 (deptsp90)
- dims 1- F1 13C, SW 236.77
- start 20160826_2323
- end   20160826_2336 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
- dims 1- F1 13C, SW 236.77
- start 20160826_2336
- end   20160826_2350 - passed
-   13C adaptive offset determined = 88.8070
-   13C adaptive SW determined = 182.6485
# Exp 6 - HSQCETGP (hsqcetgp)
- dims 2- F1 13C, SW 165.64; F2 1H, SW 12.99
- start 20160826_2350
- end   20160827_0004 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-   F1 SW changed to 182.65
-   F2 SW changed to 9.20
-   F1 1H offset changed to 0.79
-   F2 13C offset changed to 88.81
- dims 2- F1 13C, SW 182.65; F2 1H, SW 9.19
- start 20160827_0005
- end   20160827_0019 - passed
# Exp 8 - HMBCETGPL3ND (hmbcetgpl3nd)
- dims 2- F1 13C, SW 221.83; F2 1H, SW 12.02
- start 20160827_0019
- end   20160827_0101 - passed
# Exp 9 - COSY45SW (cosyqf45)
- dims 2- F1 1H, SW 10.31; F2 1H, SW 10.31
- start 20160827_0101
- end   20160827_0139 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- dims 2- F1 13C, SW 165.00; F2 1H, SW 12.02
- start 20160827_0139
- end   20160827_0258 - passed

## cq_01158 Experiment Set Ended - 20160827_0258 ##

