NMRbot_cq_03714_SampleReport.20170127_1617.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## NMRbot version 20140226 ##

## Initiated - 20170127_1617 ##

- info:
  cq_03714 in DMSO at position 201
  foldername => cq_03714.DMSO.201.20170127
  Exps => ZGCPPR,metabTOCSY,C13CPD_MMCD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND_MMCD,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 201 - passed
- DMSO solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 2 with metabTOCSY parameters
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 3 with C13CPD_MMCD parameters
-   prosol parameters loaded
-   NS changed to 2048
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters
-   prosol parameters loaded
-   NS changed to 512
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters
-   prosol parameters loaded
-   NS changed to 512
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters
-   prosol parameters loaded
-   NS changed to 4
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters
-   prosol parameters loaded
-   NS changed to 4
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND_MMCD parameters
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 10 with HSQC_TOCSY_ADIA parameters
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
- dims 1- F1 1H, SW 16.03
- start 20170127_1628
- end   20170127_1629 - passed
-   1H adaptive offset determined = 4.7498
-   1H adaptive SW determined = 8.6695
# Exp 2 - metabTOCSY (mlevph)
- dims 2- F1 1H, SW 10.21; F2 1H, SW 10.21
- start 20170127_1629
- end   20170127_1906 - passed
# Exp 3 - C13CPD_MMCD (zgpg30)
- dims 1- F1 13C, SW 248.61
- start 20170127_1907
- end   20170127_2053 - passed
# Exp 4 - C13DEPT90 (deptsp90)
- dims 1- F1 13C, SW 236.77
- start 20170127_2053
- end   20170127_2120 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
- dims 1- F1 13C, SW 236.77
- start 20170127_2120
- end   20170127_2147 - passed
-   13C adaptive offset determined = 91.9913
-   13C adaptive SW determined = 122.6140
# Exp 6 - HSQCETGP (hsqcetgp)
- dims 2- F1 13C, SW 165.64; F2 1H, SW 12.99
- start 20170127_2148
- end   20170127_2215 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-   F1 SW changed to 122.61
-   F2 SW changed to 8.67
-   F1 1H offset changed to 4.75
-   F2 13C offset changed to 91.99
- dims 2- F1 13C, SW 122.61; F2 1H, SW 8.68
- start 20170127_2215
- end   20170127_2244 - passed
# Exp 8 - HMBCETGPL3ND_MMCD (hmbcetgpl3nd)
- dims 2- F1 13C, SW 240.00; F2 1H, SW 12.02
- start 20170127_2244
- end   20170128_0007 - passed
# Exp 9 - COSY45SW (cosyqf45)
- dims 2- F1 1H, SW 10.31; F2 1H, SW 10.31
- start 20170128_0008
- end   20170128_0123 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- dims 2- F1 13C, SW 165.00; F2 1H, SW 12.02
- start 20170128_0123
- end   20170128_0359 - passed

## cq_03714 Experiment Set Ended - 20170128_0359 ##

