NMRbot_CID251562_NSC_72116_SampleReport.20181104_1157.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## NMRbot version 20140226 ##

## Initiated - 20181104_1157 ##

- info:
  CID251562_NSC_72116 in CDCl3 at position 204
  foldername => CID251562_NSC_72116.CDCl3.204.20181102
  Exps => ZGCPPR,metabTOCSY,C13CPD_MMCD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND_MMCD,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 204 - passed
- CDCl3 solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 2 with metabTOCSY parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 3 with C13CPD_MMCD parameters
-   prosol parameters loaded
-   NS changed to 4096
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters
-   prosol parameters loaded
-   NS changed to 1024
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters
-   prosol parameters loaded
-   NS changed to 1024
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND_MMCD parameters
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 10 with HSQC_TOCSY_ADIA parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
- dims 1- F1 1H, SW 16.03
- start 20181104_1209
- end   20181104_1212 - passed
-   1H adaptive offset determined = 4.7000
-   1H adaptive SW determined = 10.1749
# Exp 2 - metabTOCSY (mlevph)
- dims 2- F1 1H, SW 10.21; F2 1H, SW 10.21
- start 20181104_1212
- end   20181104_1725 - passed
# Exp 3 - C13CPD_MMCD (zgpg30)
- dims 1- F1 13C, SW 248.61
- start 20181104_1725
- end   20181104_2058 - passed
# Exp 4 - C13DEPT90 (deptsp90)
- dims 1- F1 13C, SW 236.77
- start 20181104_2058
- end   20181104_2152 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
- dims 1- F1 13C, SW 236.77
- start 20181104_2153
- end   20181104_2247 - passed
-   13C adaptive offset determined = 69.2042
-   13C adaptive SW determined = 114.4516
# Exp 6 - HSQCETGP (hsqcetgp)
- dims 2- F1 13C, SW 165.00; F2 1H, SW 12.99
- start 20181104_2247
- end   20181104_2342 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-   F1 SW changed to 114.45
-   F2 SW changed to 10.17
-   F1 1H offset changed to 4.70
-   F2 13C offset changed to 69.20
- dims 2- F1 13C, SW 114.45; F2 1H, SW 10.17
- start 20181104_2342
- end   20181105_0037 - passed
# Exp 8 - HMBCETGPL3ND_MMCD (hmbcetgpl3nd)
- dims 2- F1 13C, SW 240.00; F2 1H, SW 12.02
- start 20181105_0038
- end   20181105_0324 - passed
# Exp 9 - COSY45SW (cosyqf45)
- dims 2- F1 1H, SW 10.00; F2 1H, SW 10.00
- start 20181105_0324
- end   20181105_0556 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- dims 2- F1 13C, SW 165.00; F2 1H, SW 16.03
- start 20181105_0556
- end   20181105_1100 - passed

## CID251562_NSC_72116 Experiment Set Ended - 20181105_1100 ##

