NMRbot_NSC_71795_CID_3213_cq_05830_SampleReport.20191014_1225.txt
Status Report for Automated Sample Data Collection
## Host = kerry.nmrfam.wisc.edu ##

## NMRbot version 20140226 ##

## Initiated - 20191014_1225 ##

- info:
  NSC_71795_CID_3213_cq_05830 in DMSO at position 204
  foldername => NSC_71795_CID_3213_cq_05830.DMSO.204.20191011
  Exps => ZGCPPR,metabTOCSY,C13CPD_MMCD,C13DEPT90,C13DEPT135_MMCD,HSQCETGP,HSQCETGP,HMBCETGPL3ND_MMCD,COSY45SW,HSQC_TOCSY_ADIA
- instrument initialization - passed
- loading sample position 204 - passed
- DMSO solvent lock - passed
-   tuning probe channels - passed
-   topshim tuneb tunea - passed
- creating exp 1 with ZGCPPR parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 2 with metabTOCSY parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 3 with C13CPD_MMCD parameters
-   prosol parameters loaded
-   NS changed to 4096
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 4 with C13DEPT90 parameters
-   prosol parameters loaded
-   NS changed to 1024
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 5 with C13DEPT135_MMCD parameters
-   prosol parameters loaded
-   NS changed to 1024
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 6 with HSQCETGP parameters
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 7 with HSQCETGP parameters
-   prosol parameters loaded
-   NS changed to 8
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 8 with HMBCETGPL3ND_MMCD parameters
-   prosol parameters loaded
-   NS changed to 16
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 9 with COSY45SW parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- creating exp 10 with HSQC_TOCSY_ADIA parameters
-   prosol parameters loaded
-   NS changed to 32
-   optimizing receiver gain - passed
-   receiver gain set to 203
- experiment folders set up - passed
## Data Acquisition ##
# Exp 1 - ZGCPPR (zgcppr)
- dims 1- F1 1H, SW 16.03
- start 20191014_1235
- end   20191014_1238 - passed
-   1H adaptive offset determined = 4.7000
-   1H adaptive SW determined = 14.7329
# Exp 2 - metabTOCSY (mlevph)
- dims 2- F1 1H, SW 10.21; F2 1H, SW 10.21
- start 20191014_1238
- end   20191014_1751 - passed
# Exp 3 - C13CPD_MMCD (zgpg30)
- dims 1- F1 13C, SW 248.61
- start 20191014_1751
- end   20191014_2124 - passed
# Exp 4 - C13DEPT90 (deptsp90)
- dims 1- F1 13C, SW 236.77
- start 20191014_2124
- end   20191014_2219 - passed
# Exp 5 - C13DEPT135_MMCD (deptsp135)
- dims 1- F1 13C, SW 236.77
- start 20191014_2219
- end   20191014_2313 - passed
-   13C adaptive offset determined = 78.1986
-   13C adaptive SW determined = 153.9589
# Exp 6 - HSQCETGP (hsqcetgp)
- dims 2- F1 13C, SW 165.00; F2 1H, SW 12.99
- start 20191014_2313
- end   20191015_0008 - passed
# Exp 7 - HSQCETGP (hsqcetgp) - SWadapted
-   F1 SW changed to 153.96
-   F2 SW changed to 14.73
-   F1 1H offset changed to 4.70
-   F2 13C offset changed to 78.20
- dims 2- F1 13C, SW 153.96; F2 1H, SW 14.71
- start 20191015_0008
- end   20191015_0102 - passed
# Exp 8 - HMBCETGPL3ND_MMCD (hmbcetgpl3nd)
- dims 2- F1 13C, SW 240.00; F2 1H, SW 12.02
- start 20191015_0102
- end   20191015_0349 - passed
# Exp 9 - COSY45SW (cosyqf45)
- dims 2- F1 1H, SW 10.00; F2 1H, SW 10.00
- start 20191015_0349
- end   20191015_0621 - passed
# Exp 10 - HSQC_TOCSY_ADIA (hsqcdietgpsisp.2)
- dims 2- F1 13C, SW 165.00; F2 1H, SW 16.03
- start 20191015_0621
- end   20191015_1125 - passed

## NSC_71795_CID_3213_cq_05830 Experiment Set Ended - 20191015_1125 ##

