
New TopShim run:

version = topshim 2.0.0
date = 2021-05-06
time = 17:57:09.673
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 0.2 Hz, Target= 0.6 Hz, After= 1.4 Hz
Iteration  2: FWHM Before= 1.4 Hz, Target= 0.6 Hz, After= 1.6 Hz
Iteration  3: FWHM Before= 1.6 Hz, Target= 0.6 Hz, After= 1.4 Hz
Iteration  4: FWHM Before= 1.4 Hz, Target= 0.6 Hz, After= 1.3 Hz
Iteration  5: FWHM Before= 1.3 Hz, Target= 0.6 Hz, After= 1.3 Hz
Iteration  6: FWHM Before= 1.3 Hz, Target= 0.6 Hz, After= 1.2 Hz
Iteration  7: FWHM Before= 1.2 Hz, Target= 0.6 Hz, After= 1.4 Hz
Iteration  8: FWHM Before= 1.4 Hz, Target= 0.6 Hz, After= 0.6 Hz
Iteration  9: FWHM Before= 0.6 Hz, Target= 0.6 Hz, After= 0.6 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.765


Sample position (Shigemi) = -0.53 - 0.66 cm.

shim changes: 
Z	-81
Z2	-35
Z3	-94
Z4	+506
Z5	+335

duration = 1 min 7 sec
completed successfully
finished Thu May  6 17:58:13 2021


========================================================================
