
New TopShim run:

version = topshim 2.0.0
date = 2021-05-06
time = 21:03:48.433
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 3.4 Hz, Target= 0.3 Hz, After= 7.6 Hz
Iteration  2: FWHM Before= 7.6 Hz, Target= 0.3 Hz, After= 0.8 Hz
Iteration  3: FWHM Before= 0.8 Hz, Target= 0.3 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.613


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	+349
Z2	+41
Z3	+390
Z4	-1801
Z5	-6788

duration = 38 sec
completed successfully
finished Thu May  6 21:04:23 2021


========================================================================
