
New TopShim run:

version = topshim 2.1.0
date = 2021-12-23
time = 22:14:34.706
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 3.6 Hz, Target= 0.5 Hz, After= 1.3 Hz
Iteration 2: FWHM Before= 1.3 Hz, Target= 0.5 Hz, After= 0.3 Hz
Iteration 3: FWHM Before= 0.3 Hz, Target= 0.5 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.562


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+34
Z2	-19
Z3	+60
Z4	+389
Z5	-261
Z6	-2282
Z7	+821
Z8	+12148
X	+9
XZ	+8
Y	+43
YZ	+42

duration = 1 min 25 sec
completed successfully
finished Thu Dec 23 22:15:58 2021


========================================================================
