
New TopShim run:

version = topshim 2.0.0
date = 2021-05-11
time = 15:45:34.541
command = topshim  fine h2o_1.7mm ordmax=5 shigemi

FINE SHIMMING

Parameters:

probe = Z150329_0015
solvent = 5%DMSOinH2O_1.7mm
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.59 ppm

Results:


1D Shimming:
Iteration  1: FWHM Before= 1.7 Hz, Target= 0.2 Hz, After= 6.4 Hz
Iteration  2: FWHM Before= 6.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration  3: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After=13.6 Hz
Iteration  4: FWHM Before=13.6 Hz, Target= 0.2 Hz, After= 8.6 Hz
Iteration  5: FWHM Before= 8.6 Hz, Target= 0.2 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.82


Sample position (Shigemi) = -0.53 - 0.65 cm.

shim changes: 
Z	-59
Z2	+250
Z3	+535
Z4	-7309
Z5	-606

duration = 53 sec
completed successfully
finished Tue May 11 15:46:24 2021


========================================================================
