
New TopShim run:

version = topshim 2.1.0
date = 2021-12-21
time = 06:58:39.402
command = topshim tunea

FINE SHIMMING

Parameters:

probe = Z168276_0016
solvent = H2O+DMSO
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 4.70 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 0.9 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 3: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.496


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	+59
Z2	-3
Z3	+31
Z4	+188
Z5	-180
Z6	-1632
Z7	+680
Z8	+11528
X	+8
XZ	+8
Y	-1
YZ	+91

duration = 1 min 33 sec
completed successfully
finished Tue Dec 21 07:00:10 2021


========================================================================
